UTM : Universal Threat Manager (comme PFSense)
Proxsilas
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O Général

3 system

Mémoirevive: 2048 Mo

Processeurs : 3

Ordre d'amorcage :  Disquette, Optique, Disque dur
Accélération : Pagination imbriquée
O Affichage

Mémoire vidéo 16 Mo
Controleur graphique : VMSVGA
Serveur de bureau a distance : Désactivé
Enregistrement : Désactivé
B stockage

Controleur : IDE

Maitre primaire IDE:  PFSense-Dorian.vdi (Normal, 16,00 Gio)
Maitre secondaire IDE : ~[Lecteur optique] pfSense-CE-2.7.2-RELEASE-amd64.iso (834,15 MB)

P Audio

Pilote hote : Par défaut
Controleur: ICH ACO7

P Réseau

Interface 1: Intel PRO/1000 MT Desktop (NAT)
# usB

Controleur US OHCI, EHCI

Filtres de périphérique : 0 (0 actif)
M Dossiers partagés.
Aucun

© Description
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Copyright and Trademark Notices.

Copyright 2884-2816. Electric Sheep Fencing, LLC ("ESF™).
ALl Rights Reserved.

Copyright 2814-2823. Rubicon Gommunications, LLC d/b/a Netgate
C"Netgate™).
All Rights Reserved.

All logos, text, and content of ESF and/or Netgate, including underlying
HTHL code. designs, and graphics used and/or depicted herein are
protected under United States and international copyright and trademark
laus and treaties, and may not be used or reproduced without the prior
express uritten permission of ESF and/or Netgate.

‘pfSense” is a registered trademark of ESF. exclusively licensed to
Netgate, and may not be used without the prior express uritten

pernission of ESF and/or Netgate. A1l other trademarks shoun herein are
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Helcome to pfSense!

R Launch a shell for rescue operations
R Recover config.xnl from a previous install

<Cancel>





image4.png
How would you like to partition your disk?

A Guided UF5 Disk Setup
M Manual Disk Setup (experts)
sl Open a shell and partition by hand
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